! AP GTO Mini Control Observatory Domes file
!
! Format is 3 values for each line seperated by a comma
! Value 1 = Name of observatory (can be anything)
! Value 2 = Dome radius in meters
! Value 3 = Telescope ota offset from center of mount RA axis
! Value 4 = Telescope ota offest East - or West + from center of mount RA axis
! Value 5 = Mount height above dome base (can be negative)
! Value 6 = Dome rotation rate deg. / sec. (only used by AGF).  Set to 0.00 for NCO
! Value 7 = Mount RA and DEC axis intersection North or South from center of dome (v19.0 and newer) 
! Note: Value 7 is not used for N. de Hilster algorithm
!
!
None,0.00,0,0,0,0,0
!
SMAS,2.44,450,0,0,0,0
SMAS-BORG,2.44,650,0,0,0,0
!
!
VMC260L,1.15,430,-110,-500,6.00,100
ED130SS,1.15,280,190,-500,6.00,100
SVX080T,1.15,225,180,-500,6.00,100
Mini50,1.15,210,50,-500,6.00,100
CENTER,1.15,200,0,-500,6.00,100
!
!
PISGAH-LX200R-TV100,1.77,430,070,0,0
PISGAH-TV100-LX200R,1.77,310,-230,0,0
PISGAH-8INCH-TV100,1.77,400,160,0,0
PISGAH-TV100-8INCH,1.77,310,-130,0,0