**AGF Dome Control Manual Switch DB9 Pinouts**

Tracking Enable/Disable Switch

DSR pin 6

DTR pin 4

Pins shorted = Tracking enabled

Pins open = Tracking disabled

East West Meridian Delay Switch (used with AP hand controller)

RTS pin 7 common pin

CTS pin 8 to RTS pin 7 = No meridian delay

RI pin 9 to RTS pin 7 = West 1 hour delay

CD pin 1 to RTS pin 7 = East 1 hour delay

Switch used C&K Components A10303RNZQ

DigiKey No. CKN9822-ND

Rotary switch 3 position

Open/Close Mount and AGF Dome Controller serial ports

RX pin 2 to RTS pin 7 = Momentary short sends break

*AP GTO Mini Control version 8.4 and above.*

